Bound, Perkins 1 Digital, Sun

DHCPv6 and Extensions

Jim Bound Charles E. Perkins bound@zk3.dec.com cperkins@eng.sun.com http://www.srvloc.org/~charliep

Bound, Perkins 2 Digital, Sun

DHCP Solicit Message Format

Bound, Perkins 3 Digital, Sun

DHCP Advertise Message Format

Bound, Perkins 4 Digital, Sun

DHCP Solicit/Advertise Message Flow

Figure 1: Getting a DHCP Server address

Bound, Perkins 5 Digital, Sun

DHCP Request Message Format

Bound, Perkins 6 Digital, Sun

DHCP Reply Message Format

Bound, Perkins 7 Digital, Sun

DHCP Request/Reply Message Flow

Figure 2: Getting a DHCP Server address

Bound, Perkins 8 Digital, Sun

DHCP Release Message Format

Bound, Perkins 9 Digital, Sun

DHCP Reconfigure Message Format

Bound, Perkins 10 Digital, Sun

Changes since last IETF

ffl preference field always present ffl relays may use configured DHCP Server addresses ffl Request retransmission after Reconfigure ffl servers MAY reallocate resources after failure to renew ffl Eliminated the ’N’ bit from the DHCP Request message. ffl Added a pfx-size to the DHCP Solicit message. ffl Deleted transaction-ID from client bindings. ffl silently discard Reconfigure if waiting for Reply. ffl server MAY be identify client bindings by MAC address ffl New formats for SLP options

Bound, Perkins 11 Digital, Sun

ffl New platform-specific extensions ffl relay handling for ICMP ffl Various clarifications, typos and fixups.