Perkins, Johnson 1 Sun, CMU

Special Tunnels

Charles E. Perkins cperkins@eng.sun.com http://www.srvloc.org/~charliep

David B. Johnson dbj@cs.cmu.edu http://www.monarch.cs.cmu.edu/

Perkins, Johnson 2 Sun, CMU

Special Tunnels

ffl Problem: an old FA could send stray MN packets to Home Network, but routing loops would be created if HA thinks that the MN is still using the care-of address at the old FA.

ffl Solution: the old FA tunnels the packet to the MN’s Home address. Then:

– inner source = Correspondent Node – outer source = old FA – inner dest = Mobile Node – outer dest = Mobile Node ffl If Home Agent detects that inner dest == outer dest and the mobile node is NOT at the old FA’s care-of address, then it can tunnel the packet again